**PRB Data Flag Key**

No flag = is a valid sample

ND = Non-detect. For H2S, CH4, and C2H6, these are negative values. For benzene and toluene, these are values less than 0.001 ppb. For statistical purposes, define value as zero.

MD = Detected, but less than the method detection limit (MDL). For statistical purposes, define value as half of MDL.

II = Instrument Issue, data is invalidated. No value reported, and should not be included in statistical analysis.

Cal = Calibration performed on instrument. No value reported, and should not be included in statistical analysis.